Global Talker

Motorola L2000i WAP Setup Port #: 9201 IP Address: 205.179.001.045

1. Press "Menu"
2. Select Access Internet
3. While connecting to the server, Press and Hold "Menu" Until the Browser Menu appears.

1. In the Browser Menu, scroll down to Setup

1. Press "OK" to the Setup Menu

1. Choose Primary Data and Press "View"

1. Choose IP Address and Press "Edit"

1. Enter the IP Address: 205.179.001.045
2. Press "OK" to get back to Primary Data Menu

1. Scroll down to Port # and Press "OK"
2. Enter Port #: 9201
3. Press "OK" to get back to Primary Data Menu
4. Press "Back" to get back to Setup Menu

1. Scroll down to Data Info and Press "View"
2. Select Phone # and Press "Edit". Enter your local access number and Press "OK".
3. Scroll down to User and Press "Edit". Enter your Globaltalker Member Login ID and Press "OK".
4. Scroll down to Password and Press "Edit". Enter your Globaltalker™ Member Password and Press "OK".
5. Scroll down to Baud Rate and Press "Edit". Choose 9600 and Press "OK".
6. Scroll down to Idle Time Out and Press "Edit". Enter 180 and Press "OK".
7. Scroll down to Line Type and Press "Edit". Choose Modem and Press "OK".

1. Exit WAP connection
2. Turn off the cellular phone
3. Turn it back on and you are ready to use Globaltalker WAP services.

Globaltalker.com ©2000-2001 All Rights Reserved.